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	1
	A periodic wave has a frequency of 4 GHz. The period time T for this wave is:
	2
	The Boolean expression    represents:

	
	a. 0.25 ns
	b. 0.25 ps
	
	a. OR gate
	b. NOR gate

	
	c. 0.25 ms
	d. 0.25 Gs
	
	c. XNOR gate
	d. XOR gate



	3
	The decimal number 67.5 is equivalent to the following binary number:
	4
	Which of the following is an unweighted code?

	
	a. 01000011.1
	b. 10000000.1
	
	a. Decimal
	b. Gray

	
	c. 10000000.01
	d. 01000011.01
	
	c. Octal
	d. All of the above



	5
	The BCD number 1000 0010 0111 1001 is equivalent to the following decimal number:
	6
	The binary number 00010101.01 is equivalent to the following decimal number:

	
	a. 9728
	b. 8279
	
	a. 21.5
	b. 36.25

	
	c. 8475
	d. None of the above
	
	c. 36.5
	d. 21.25



	7
	The hexadecimal number 1F is equivalent to the following decimal number:
	8
	The 2's complement of the number 00110101 is:

	
	a. 31
	b. 16
	
	a. 11001010
	b. 11001101

	
	c. 115
	d. None of the above
	
	c. 11001011
	d. None of the above



	9
	Data can be transmitted by either serial transfer or parallel transfer. Which of the following statement is true?

	
	a. serial is faster than parallel.
	b. parallel is faster than serial.

	
	c. parallel and serial are the same.
	d. None of the above



	10
	The following truth table is for: 
		A      B
	Output

	0      0
	1

	0      1
	0

	1      0
	0

	1      1
	0




	
	a. XOR
	b. NAND

	
	c. NOR
	d. XNOR
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